Next: ARC Options, Previous: Adapteva Epiphany Options, Up: Submodel Options [Contents][Index]

#### 3.19.3 AMD GCN Options

These options are defined specifically for the AMD GCN port.

`-march=gpu`
`-mtune=gpu`

  Set architecture type or tuning for gpu. Supported values for gpu are

  ‘`fiji`’

    Compile for GCN3 Fiji devices (gfx803). Support deprecated; availablility depends on how GCC has been configured, see `--with-arch` and `--with-multilib-list`.

  ‘`gfx900`’

    Compile for GCN5 Vega 10 devices (gfx900).

  ‘`gfx906`’

    Compile for GCN5 Vega 20 devices (gfx906).

  ‘`gfx908`’

    Compile for CDNA1 Instinct MI100 series devices (gfx908).

  ‘`gfx90a`’

    Compile for CDNA2 Instinct MI200 series devices (gfx90a).

  ‘`gfx90c`’

    Compile for GCN5 Vega 7 devices (gfx90c).

  ‘`gfx1030`’

    Compile for RDNA2 gfx1030 devices (GFX10 series).

  ‘`gfx1036`’

    Compile for RDNA2 gfx1036 devices (GFX10 series).

  ‘`gfx1100`’

    Compile for RDNA3 gfx1100 devices (GFX11 series).

  ‘`gfx1103`’

    Compile for RDNA3 gfx1103 devices (GFX11 series).

`-msram-ecc=on`
`-msram-ecc=off`
`-msram-ecc=any`

  Compile binaries suitable for devices with the SRAM-ECC feature enabled, disabled, or either mode. This feature can be enabled per-process on some devices. The compiled code must match the device mode. The default is ‘`any`’, for devices that support it.

`-mstack-size=bytes`

  Specify how many bytes of stack space will be requested for each GPU thread (wave-front). Beware that there may be many threads and limited memory available. The size of the stack allocation may also have an impact on run-time performance. The default is 32KB when using OpenACC or OpenMP, and 1MB otherwise.

`-mxnack=on`
`-mxnack=off`
`-mxnack=any`

  Compile binaries suitable for devices with the XNACK feature enabled, disabled, or either mode. Some devices always require XNACK and some allow the user to configure XNACK. The compiled code must match the device mode. The default is ‘`-mxnack=any`’ on devices that support Unified Shared Memory, and ‘`-mxnack=no`’ otherwise.

Next: ARC Options, Previous: Adapteva Epiphany Options, Up: Submodel Options [Contents][Index]