This is porting.info, produced by makeinfo version 6.7 from
porting.texi.

Copyright (C) 1993, 1994, 1995 Cygnus Support

   Permission is granted to make and distribute verbatim copies of this
manual provided the copyright notice and this permission notice are
preserved on all copies.

   Permission is granted to copy and distribute modified versions of
this manual under the conditions for verbatim copying, provided also
that the entire resulting derived work is distributed under the terms of
a permission notice identical to this one.

   Permission is granted to copy and distribute translations of this
manual into another language, under the above conditions for modified
versions.
START-INFO-DIR-ENTRY
START-INFO-DIR-ENTRY
* Embed with GNU: (porting-).         Embed with GNU
END-INFO-DIR-ENTRY
END-INFO-DIR-ENTRY

   Copyright (C) 1993, 1994, 1995 Cygnus Support

   Permission is granted to make and distribute verbatim copies of this
manual provided the copyright notice and this permission notice are
preserved on all copies.

   Permission is granted to copy and distribute modified versions of
this manual under the conditions for verbatim copying, provided also
that the entire resulting derived work is distributed under the terms of
a permission notice identical to this one.

   Permission is granted to copy and distribute translations of this
manual into another language, under the above conditions for modified
versions.


File: porting.info,  Node: Top,  Next: Libgloss,  Up: (dir)

Embed with GNU
**************

*Rough Draft*

   The goal of this document is to gather all the information needed to
port the GNU tools to a new embedded target in one place.  This will
duplicate some info found in the other manual for the GNU tools, but
this should be all you'll need.

* Menu:

* Libgloss::            Libgloss, a library of board support packages.
* GCC::                 Porting GCC/G++ to a new embedded target.
* Libraries::           Making Newlib run on an new embedded target.
* GDB::                 Making GDB understand a new back end.
* Binutils::            Using the GNU binary utilities.
* Code Listings::       Listings of the commented source code from the
                        text.


File: porting.info,  Node: Libgloss,  Next: GCC,  Prev: Top,  Up: Top

1 Libgloss
**********

Libgloss is a library for all the details that usually get glossed over.
This library refers to things like startup code, and usually I/O support
for 'gcc' and 'C library'.  The C library used through out this manual
is 'newlib'.  Newlib is a ANSI conforming C library developed by Cygnus
Support.  Libgloss could easily be made to support other C libraries,
and it can be used standalone as well.  The standalone configuration is
typically used when bringing up new hardware, or on small systems.

   For a long time, these details were part of newlib.  This approach
worked well when a complete tool chain only had to support one system.
A tool chain refers to the series of compiler passes required to produce
a binary file that will run on an embedded system.  For C, the passes
are cpp, gcc, gas, ld.  Cpp is the preprocessor, which process all the
header files and macros.  Gcc is the compiler, which produces assembler
from the processed C files.  Gas assembles the code into object files,
and then ld combines the object files and binds the code to addresses
and produces the final executable image.

   Most of the time a tool chain does only have to support one target
execution environment.  An example of this would be a tool chain for the
AMD 29k processor family.  All of the execution environments for this
processor have the same interface, the same memory map, and the same I/O
code.  In this case all of the support code is under newlib/libc/sys.
Libgloss's creation was forced initially because of the 'cpu32'
processor family.  There are many different execution environments for
this line, and they vary wildly.  newlib itself has only a few
dependencies that it needs for each target.  These are explained later
in this doc.  The hardware dependent part of newlib was reorganized into
a separate directory structure within newlib called the stub dirs.  It
was initially called this because most of the routines newlib needs for
a target were simple stubs that do nothing, but return a value to the
application.  They only exist so the linker can produce a final
executable image.  This work was done during the early part of 1993.

   After a while it became apparent that this approach of isolating the
hardware and systems files together made sense.  Around this same time
the stub dirs were made to run standalone, mostly so it could also be
used to support GDB's remote debugging needs.  At this time it was
decided to move the stub dirs out of newlib and into its own separate
library so it could be used standalone, and be included in various other
GNU tools without having to bring in all of newlib, which is large.  The
new library is called Libgloss, for Gnu Low-level OS support.

* Menu:

* Supported targets::           What targets libgloss currently
                                supports.
* Building libgloss::           How to configure and built libgloss
                                for a target.
* Board support::               How to add support for a new board.
* Build System Internals::      How the libgloss build system works.


File: porting.info,  Node: Supported targets,  Next: Building libgloss,  Prev: Libgloss,  Up: Libgloss

1.1 Supported Targets
=====================

Currently libgloss is being used for at least the following targets:

* Menu:

* Blackfin::                    Analog Devices, Inc. Blackfin processor.
* Sparclite::                   Fujitsu's sparclite.
* CPU32::                       Various m68k based targets.
* Mips::                        Mips code based targets.
* PA-RISC::                     Precision Risc Organization..


File: porting.info,  Node: Blackfin,  Next: Sparclite,  Up: Supported targets

1.1.1 Blackfin Targets Supported
--------------------------------

This is for the Analog Devices, Inc.  Blackfin family of processors.
Currently this covers all versions except for the BF535.


File: porting.info,  Node: Sparclite,  Next: CPU32,  Prev: Blackfin,  Up: Supported targets

1.1.2 Sparclite Targets Supported
---------------------------------

This is for the Fujitsu Sparclite family of processors.  Currently this
covers the ex930, ex931, ex932, ex933, and the ex934.  In addition to
the I/O code a startup file, this has a GDB debug-stub that gets linked
into your application.  This is an exception handler style debug stub.
For more info, see the section on Porting GDB. *note Porting GDB: GDB.

   The Fujitsu eval boards use a host based terminal program to load and
execute programs on the target.  This program, 'pciuh' is relatively new
(in 1994) and it replaced the previous ROM monitor which had the shell
in the ROM. GDB uses the the GDB remote protocol, the relevant source
files from the gdb sources are remote-sparcl.c.  The debug stub is part
of libgloss and is called sparcl-stub.c.


File: porting.info,  Node: CPU32,  Next: Mips,  Prev: Sparclite,  Up: Supported targets

1.1.3 Motorola CPU32 Targets supported
--------------------------------------

This refers to Motorola's m68k based CPU32 processor family.  The crt0.S
startup file should be usable with any target environment, and it's
mostly just the I/O code and linker scripts that vary.  Currently there
is support for the Motorola MVME line of 6U VME boards and IDP line of
eval boards.  All of the Motorola VME boards run 'Bug', a ROM based
debug monitor.  This monitor has the feature of using user level traps
to do I/O, so this code should be portable to other MVME boards with
little if any change.  The startup file also can remain unchanged.
About the only thing that varies is the address for where the text
section begins.  This can be accomplished either in the linker script,
or on the command line using the '-Ttext [address]'.

   There is also support for the 'rom68k' monitor as shipped on
Motorola's IDP eval board line.  This code should be portable across the
range of CPU's the board supports.  There is also GDB support for this
target environment in the GDB source tree.  The relevant files are
gdb/monitor.c, monitor.h, and rom58k-rom.c.  The usage of these files is
discussed in the GDB section.


File: porting.info,  Node: Mips,  Next: PA-RISC,  Prev: CPU32,  Up: Supported targets

1.1.4 Mips core Targets Supported
---------------------------------

The Crt0 startup file should run on any mips target that doesn't require
additional hardware initialization.  The I/O code so far only supports a
custom LSI33k based RAID disk controller board.  It should easy to
change to support the IDT line of eval boards.  Currently the two
debugging protocols supported by GDB for mips targets is IDT's mips
debug protocol, and a customized hybrid of the standard GDB remote
protocol and GDB's standard ROM monitor support.  Included here is the
debug stub for the hybrid monitor.  This supports the LSI33k processor,
and only has support for the GDB protocol commands 'g', 'G', 'm', 'M',
which basically only supports the register and memory reading and
writing commands.  This is part of libgloss and is called lsi33k-stub.c.

   The crt0.S should also work on the IDT line of eval boards, but has
only been run on the LSI33k for now.  There is no I/O support for the
IDT eval board at this time.  The current I/O code is for a customized
version of LSI's 'pmon' ROM monitor.  This uses entry points into the
monitor, and should easily port to other versions of the pmon monitor.
Pmon is distributed in source by LSI.


File: porting.info,  Node: PA-RISC,  Prev: Mips,  Up: Supported targets

1.1.5 PA-RISC Targets Supported
-------------------------------

This supports the various boards manufactured by the HP-PRO consortium.
This is a group of companies all making variations on the PA-RISC
processor.  Currently supported are ports to the WinBond 'Cougar' board
based around their w89k version of the PA. Also supported is the Oki
op50n processor.

   There is also included, but never built an unfinished port to the HP
743 board.  This board is the main CPU board for the HP700 line of
industrial computers.  This target isn't exactly an embedded system, in
fact it's really only designed to load and run HP-UX. Still, the crt0.S
and I/O code are fully working.  It is included mostly because their is
a barely functioning exception handler GDB debug stub, and I hope
somebody could use it.  The other PRO targets all use GDB's ability to
talk to ROM monitors directly, so it doesn't need a debug stub.  There
is also a utility that will produce a bootable file by HP's ROM monitor.
This is all included in the hopes somebody else will finish it.  :-)

   Both the WinBond board and the Oki board download srecords.  The
WinBond board also has support for loading the SOM files as produced by
the native compiler on HP-UX. WinBond supplies a set of DOS programs
that will allow the loading of files via a bidirectional parallel port.
This has never been tested with the output of GNU SOM, as this manual is
mostly for Unix based systems.


File: porting.info,  Node: Building libgloss,  Next: Board support,  Prev: Supported targets,  Up: Libgloss

1.2 Configuring and building libgloss.
======================================

Libgloss uses an autoconf based script to configure.  Autoconf scripts
are portable shell scripts that are generated from a configure.ac file.
Configure input scripts are based themselves on m4.  Most configure
scripts run a series of tests to determine features the various
supported features of the target.  For features that can't be determined
by a feature test, a makefile fragment is merged in.  The configure
process leaves creates a Makefile in the build directory.  For libgloss,
there are only a few configure options of importance.  These are -target
and -srcdir.

   Typically libgloss is built in a separate tree just for objects.  In
this manner, it's possible to have a single source tree, and multiple
object trees.  If you only need to configure for a single target
environment, then you can configure in the source tree.  The argument
for -target is a config string.  It's usually safest to use the full
canonical opposed to the target alias.  So, to configure for a CPU32
(m68k) with a separate source tree, use:

     ../src/libgloss/configure --verbose --target m68k-coff

   The configure script is in the source tree.  When configure is
invoked it will determine its own source tree, so the -srcdir is would
be redundant here.

   Once libgloss is configured, 'make' is sufficient to build it.  The
default values for 'Makefiles' are typically correct for all supported
systems.  The test cases in the testsuite will also built automatically
as opposed to a 'make check', where test binaries aren't built till test
time.  This is mostly cause the libgloss testsuites are the last thing
built when building the entire GNU source tree, so it's a good test of
all the other compilation passes.

   The default values for the Makefiles are set in the Makefile fragment
merged in during configuration.  This fragment typically has rules like

     CC_FOR_TARGET = `if [ -f $${OBJROOT}/gcc/xgcc ] ; \
     	then echo ${OBJROOT}/gcc/xgcc -B${OBJROOT}/gcc/ ; \
     	else t='${program_transform_name}'; echo gcc | sed -e '' $$t ; fi`

   Basically this is a runtime test to determine whether there are
freshly built executables for the other main passes of the GNU tools.
If there isn't an executable built in the same object tree, then
_transformed_the generic tool name (like gcc) is transformed to the name
typically used in GNU cross compilers.  The names are typically based on
the target's canonical name, so if you've configured for 'm68k-coff' the
transformed name is 'm68k-coff-gcc' in this case.  If you install with
aliases or rename the tools, this won't work, and it will always look
for tools in the path.  You can force the a different name to work by
reconfiguring with the '--program-transform-name' option to configure.
This option takes a sed script like this '-e s,^,m68k-coff-,' which
produces tools using the standard names (at least here at Cygnus).

   The search for the other GNU development tools is exactly the same
idea.  This technique gets messier when build options like
'-msoft-float' support are used.  The Makefile fragments set the
'MUTILIB' variable, and if it is set, the search path is modified.  If
the linking is done with an installed cross compiler, then none of this
needs to be used.  This is done so libgloss will build automatically
with a fresh, and uninstalled object tree.  It also makes it easier to
debug the other tools using libgloss's test suites.


File: porting.info,  Node: Board support,  Next: Build System Internals,  Prev: Building libgloss,  Up: Libgloss

1.3 Adding Support for a New Board
==================================

This section explains how to add support for a new board to libgloss.
In order to add support for a board, you must already have developed a
toolchain for the target architecture.

   All of the changes you will make will be in the subdirectory named
after the architecture used by your board.  For example, if you are
developing support for a new ColdFire board, you will modify files in
the 'm68k' subdirectory, as that subdirectory contains support for all
68K devices, including architecture variants like ColdFire.

   In general, you will be adding three components: a 'crt0.S' file
(*note Crt0::), a linker script (*note Linker Scripts::), and a hardware
support library.  Each should be prefixed with the name of your board.
For example, if you ard adding support for a new Surf board, then you
will be adding the assembly 'surf-crt0.S' (which will be assembled into
'surf-crt0.o'), the linker script 'surf.ld', and other C and assembly
files which will be combined into the hardware support library
'libsurf.a'.

   You should modify 'Makefile.in' to define new variables corresponding
to your board.  Although there is some variation between architectures,
the general convention is to use the following format:

     # The name of the crt0.o file.
     SURF_CRT0    = surf-crt0.o
     # The name of the linker script.
     SURF_SCRIPTS = surf.ld
     # The name of the hardware support library.
     SURF_BSP     = libsurf.a
     # The object files that make up the hardware support library.
     SURF_OBJS    = surf-file1.o surf-file2.o
     # The name of the Makefile target to use for installation.
     SURF_INSTALL = install-surf

   Then, you should create the '${SURF_BSP}' and '${SURF_INSTALL}' make
targets.  Add '${SURF_CRT0}' to the dependencies for the 'all' target
and add '${SURF_INSTALL}' to the dependencies for the 'install' target.
Now, when libgloss is built and installed, support for your BSP will be
installed as well.


File: porting.info,  Node: Build System Internals,  Prev: Board support,  Up: Libgloss

1.4 Build System Internals
==========================

As noted previously, Libgloss uses GNU Autotools (*note GNU Autoconf:
(autoconf)Top. & *note GNU Automake: (automake)Top.) to build.  *note
GNU Libtool: (libtool)Top. is not used as Libgloss only produces objects
and static archives, and *note GNU Automake: (automake)Top. is capable
of handling that.

   If you're editing any of these files and want to regenerate them,
simply run 'autoreconf'.  It will take care of the rest.

   Tool versions are strictly controlled.  You must use GNU Autoconf
2.69 and GNU Automake 1.15.1 to generate the build files.  If your
system does not include them, you can manually download and install them
into your home directory.

   All of the common configure logic lives in 'configure.ac'.  It checks
for supported targets and creates the makefiles.  Any architecture that
wishes to run custom configure tests should store them in 'acinclude.m4'
in their respective subdirectory and then use 'm4_include' in
'configure.ac'.  Make sure to avoid running excessive tests for all
targets, and avoid using generic names that can collide with other
architectures - the build uses a flat namespace that is shared among
everyone.

   Libgloss has partially converted to *note GNU Automake:
(automake)Top.  The top-level directory uses it with 'Makefile.am', as
do a few subdirectories with their 'Makefile.inc' fragments.  The other
subdirectories still use hand written 'Makefile.in' files.  One day,
they should get converted over too.  Patches welcome!

   For directories that have converted to *note GNU Automake:
(automake)Top, a non-recursive build is used.  That means only a single
Makefile is created in the top-level, and no Makefiles are created in
subdirectories.  Make must be run in the top-level at all times.

   The 'config/*.mh' and 'config/*.mt' files are only used by the non-
Automake files (i.e., the 'Makefile.in' files).  They can be ignored for
any target that has migrated to *note GNU Automake: (automake)Top.

   Libgloss automatically builds itself for all multilib configurations
that the active toolchain supports.  This logic is provided by common
code from the combined toolchain source tree.


File: porting.info,  Node: GCC,  Next: Libraries,  Prev: Libgloss,  Up: Top

2 Porting GCC
*************

Porting GCC requires two things, neither of which has anything to do
with GCC. If GCC already supports a processor type, then all the work in
porting GCC is really a linker issue.  All GCC has to do is produce
assembler output in the proper syntax.  Most of the work is done by the
linker, which is described elsewhere.

   Mostly all GCC does is format the command line for the linker pass.
The command line for GCC is set in the various config subdirectories of
gcc.  The options of interest to us are 'CPP_SPEC' and 'STARTFILE_SPEC'.
CPP_SPEC sets the builtin defines for your environment.  If you support
multiple environments with the same processor, then OS specific defines
will need to be elsewhere.

   'STARTFILE_SPEC'

   Once you have linker support, GCC will be able to produce a fully
linked executable image.  The only _part_ of GCC that the linker wants
is a crt0.o, and a memory map.  If you plan on running any programs that
do I/O of any kind, you'll need to write support for the C library,
which is described elsewhere.

* Menu:

* Overview::            An overview as to the compilation passes.
* Options::             Useful GCC options for embedded systems.


File: porting.info,  Node: Overview,  Next: Options,  Up: GCC

2.1 Compilation passes
======================

GCC by itself only compiles the C or C++ code into assembler.  Typically
GCC invokes all the passes required for you.  These passes are cpp, cc1,
gas, ld.  'cpp' is the C preprocessor.  This will merge in the include
files, expand all macros definitions, and process all the '#ifdef'
sections.  To see the output of ccp, invoke gcc with the '-E' option,
and the preprocessed file will be printed on the stdout.  cc1 is the
actual compiler pass that produces the assembler for the processed file.
GCC is actually only a driver program for all the compiler passes.  It
will format command line options for the other passes.  The usual
command line GCC uses for the final link phase will have LD link in the
startup code and additional libraries by default.

   GNU AS started its life to only function as a compiler pass, but
these days it can also be used as a source level assembler.  When used
as a source level assembler, it has a companion assembler preprocessor
called 'gasp'.  This has a syntax similar to most other assembler macros
packages.  GAS emits a relocatable object file from the assembler
source.  The object file contains the executable part of the
application, and debug symbols.

   LD is responsible for resolving the addresses and symbols to
something that will be fully self-contained.  Some RTOS's use
relocatable object file formats like 'a.out', but more commonly the
final image will only use absolute addresses for symbols.  This enables
code to be burned into PROMS as well.  Although LD can produce an
executable image, there is usually a hidden object file called 'crt0.o'
that is required as startup code.  With this startup code and a memory
map, the executable image will actually run on the target environment.
*note Startup Files: Crt0.

   The startup code usually defines a special symbol like '_start' that
is the default base address for the application, and the first symbol in
the executable image.  If you plan to use any routines from the standard
C library, you'll also need to implement the functions that this library
is dependent on.  *note Porting Newlib: Libraries.


File: porting.info,  Node: Options,  Prev: Overview,  Up: GCC

Options for the various development tools are covered in more detail
elsewhere.  Still, the amount of options can be an overwhelming amount
of stuff, so the options most suited to embedded systems are summarized
here.  If you use GCC as the main driver for all the passes, most of the
linker options can be passed directly to the compiler.  There are also
GCC options that control how the GCC driver formats the command line
arguments for the linker.

* Menu:

* GCC Options::         Options for the compiler.
* GAS Options::         Options for the assembler.
* LD Options::          Options for the linker.


File: porting.info,  Node: GCC Options,  Next: GAS Options,  Up: Options

Most of the GCC options that we're interested control how the GCC driver
formats the options for the linker pass.

'-nostartfiles'
'-nostdlib'
'-Xlinker'
     Pass the next option directly to the linker.

'-v'
'-fpic'


File: porting.info,  Node: GAS Options,  Next: LD Options,  Prev: GCC Options,  Up: Options


File: porting.info,  Node: LD Options,  Prev: GAS Options,  Up: Options


File: porting.info,  Node: Libraries,  Next: GDB,  Prev: GCC,  Up: Top

3 Porting newlib
****************

* Menu:

* Crt0::                Crt0.S.
* Linker Scripts::      Linker scripts for memory management.
* What to do now::      Tricks for manipulating formats.
* Libc::                Making libc work.


File: porting.info,  Node: Crt0,  Next: Linker Scripts,  Up: Libraries

3.1 Crt0, the main startup file
===============================

To make a program that has been compiled with GCC to run, you need to
write some startup code.  The initial piece of startup code is called a
crt0.  (C RunTime 0) This is usually written in assembler, and its
object gets linked in first, and bootstraps the rest of the application
when executed.  This file needs to do the following things.

  1. Initialize anything that needs it.  This init section varies.  If
     you are developing an application that gets download to a ROM
     monitor, then there is usually no need for any special
     initialization.  The ROM monitor handles it for you.

     If you plan to burn your code in a ROM, then the crt0 typically has
     to do all the hardware initialization that is required to run an
     application.  This can include things like initializing serial
     ports or run a memory check.  It all depends on the hardware.

  2. Zero the BSS section.  This is for uninitialized data.  All the
     addresses in this section need to be initialized to zero so that
     programs that forget to check new variables default value will get
     unpredictable results.

  3. Call main() This is what basically starts things running.  If your
     ROM monitor supports it, then first setup argc and argv for command
     line arguments and an environment pointer.  Then branch to main().
     For G++ the the main routine gets a branch to __main inserted by
     the code generator at the very top.  __main() is used by G++ to
     initialize its internal tables.  __main() then returns back to your
     original main() and your code gets executed.

  4. Call exit() After main() has returned, you need to cleanup things
     and return control of the hardware from the application.  On some
     hardware, there is nothing to return to, especially if your program
     is in ROM. Sometimes the best thing to do in this case is do a
     hardware reset, or branch back to the start address all over again.

     When there is a ROM monitor present, usually a user trap can be
     called and then the ROM takes over.  Pick a safe vector with no
     side effects.  Some ROMs have a builtin trap handler just for this
     case.
   portable between all the m68k based boards we have here.  *note
Example Crt0.S: crt0.S.

     /* ANSI concatenation macros.  */

     #define CONCAT1(a, b) CONCAT2(a, b)
     #define CONCAT2(a, b) a ## b
   These we'll use later.

     /* These are predefined by new versions of GNU cpp.  */

     #ifndef __USER_LABEL_PREFIX__
     #define __USER_LABEL_PREFIX__ _
     #endif

     /* Use the right prefix for global labels.  */
     #define SYM(x) CONCAT1 (__USER_LABEL_PREFIX__, x)


   These macros are to make this code portable between both _COFF_ and
_a.out_.  _COFF_ always has an _ (UNDERLINE) prepended on the front of
all global symbol names.  _a.out_ has none.

     #ifndef __REGISTER_PREFIX__
     #define __REGISTER_PREFIX__
     #endif

     /* Use the right prefix for registers.  */
     #define REG(x) CONCAT1 (__REGISTER_PREFIX__, x)

     #define d0 REG (d0)
     #define d1 REG (d1)
     #define d2 REG (d2)
     #define d3 REG (d3)
     #define d4 REG (d4)
     #define d5 REG (d5)
     #define d6 REG (d6)
     #define d7 REG (d7)
     #define a0 REG (a0)
     #define a1 REG (a1)
     #define a2 REG (a2)
     #define a3 REG (a3)
     #define a4 REG (a4)
     #define a5 REG (a5)
     #define a6 REG (a6)
     #define fp REG (fp)
     #define sp REG (sp)

   This is for portability between assemblers.  Some register names have
a % or $ prepended to the register name.

     /*
      * Set up some room for a stack. We just grab a chunk of memory.
      */
     	.set	stack_size, 0x2000
     	.comm	SYM (stack), stack_size

   Set up space for the stack.  This can also be done in the linker
script, but it typically gets done here.

     /*
      * Define an empty environment.
      */
             .data
             .align 2
     SYM (environ):
             .long 0

   Set up an empty space for the environment.  This is bogus on any most
ROM monitor, but we setup a valid address for it, and pass it to main.
At least that way if an application checks for it, it won't crash.

      	.align	2
     	.text
     	.global SYM (stack)

     	.global SYM (main)
     	.global SYM (exit)
     /*
      * This really should be __bss_start, not SYM (__bss_start).
      */
     	.global __bss_start

   Setup a few global symbols that get used elsewhere.  __BSS_START
needs to be unchanged, as it's setup by the linker script.

     /*
      * start -- set things up so the application will run.
      */
     SYM (start):
     	link	a6, #-8
     	moveal	#SYM (stack) + stack_size, sp

     /*
      * zerobss -- zero out the bss section
      */
     	moveal	#__bss_start, a0
     	moveal	#SYM (end), a1
     1:
     	movel	#0, (a0)
     	leal	4(a0), a0
     	cmpal	a0, a1
     	bne	1b

   The global symbol 'start' is used by the linker as the default
address to use for the '.text' section.  then it zeros the '.bss'
section so the uninitialized data will all be cleared.  Some programs
have wild side effects from having the .bss section let uncleared.
Particularly it causes problems with some implementations of 'malloc'.

     /*
      * Call the main routine from the application to get it going.
      * main (argc, argv, environ)
      * We pass argv as a pointer to NULL.
      */
             pea     0
             pea     SYM (environ)
             pea     sp@(4)
             pea     0
     	jsr	SYM (main)
     	movel	d0, sp@-

   Setup the environment pointer and jump to 'main()'.  When 'main()'
returns, it drops down to the 'exit' routine below.

     /*
      * _exit -- Exit from the application. Normally we cause a user trap
      *          to return to the ROM monitor for another run.
      */
     SYM (exit):
     	trap	#0

   Implementing 'exit' here is easy.  Both the 'rom68k' and 'bug' can
handle a user caused exception of 'zero' with no side effects.  Although
the 'bug' monitor has a user caused trap that will return control to the
ROM monitor, this solution has been more portable.


File: porting.info,  Node: Linker Scripts,  Next: What to do now,  Prev: Crt0,  Up: Libraries

3.2 Linker scripts for memory management
========================================

The linker script sets up the memory map of an application.  It also
sets up default values for variables used elsewhere by sbrk() and the
crt0.  These default variables are typically called '_bss_start' and
'_end'.

   For G++, the constructor and destructor tables must also be setup
here.  The actual section names vary depending on the object file
format.  For 'a.out' and 'coff', the three main sections are '.text',
'.data', and '.bss'.

   Now that you have an image, you can test to make sure it got the
memory map right.  You can do this by having the linker create a memory
map (by using the '-Map' option), or afterwards by using 'nm' to check a
few critical addresses like 'start', 'bss_end', and '_etext'.

   Here's a breakdown of a linker script for a m68k based target board.
See the file 'libgloss/m68k/idp.ld', or go to the appendixes in the end
of the manual.  *note Example Linker Script: idp.ld.

     STARTUP(crt0.o)
     OUTPUT_ARCH(m68k)
     INPUT(idp.o)
     SEARCH_DIR(.)
     __DYNAMIC  =  0;

   The 'STARTUP' command loads the file specified so that it's first.
In this case it also doubles to load the file as well, because the
m68k-coff configuration defaults to not linking in the crt0.o by
default.  It assumes that the developer probably has their own crt0.o.
This behavior is controlled in the config file for each architecture.
It's a macro called 'STARTFILE_SPEC', and if it's set to 'null', then
when 'gcc' formats its command line, it doesn't add 'crto.o'.  Any file
name can be specified here, but the default is always 'crt0.o'.

   Course if you only use 'ld' to link, then the control of whether or
not to link in 'crt0.o' is done on the command line.  If you have
multiple crto files, then you can leave this out all together, and link
in the 'crt0.o' in the makefile, or by having different linker scripts.
Sometimes this is done for initializing floating point optionally, or to
add device support.

   The 'OUTPUT_ARCH' sets architecture the output file is for.

   'INPUT' loads in the file specified.  In this case, it's a relocated
library that contains the definitions for the low-level functions need
by libc.a.  This could have also been specified on the command line, but
as it's always needed, it might as well be here as a default.
'SEARCH_DIR' specifies the path to look for files, and '_DYNAMIC' means
in this case there are no shared libraries.

     /*
      * Setup the memory map of the MC68ec0x0 Board (IDP)
      * stack grows up towards high memory. This works for
      * both the rom68k and the mon68k monitors.
      */
     MEMORY
     {
       ram     : ORIGIN = 0x10000, LENGTH = 2M
     }

   This specifies a name for a section that can be referred to later in
the script.  In this case, it's only a pointer to the beginning of free
RAM space, with an upper limit at 2M. If the output file exceeds the
upper limit, it will produce an error message.

     /*
      * stick everything in ram (of course)
      */
     SECTIONS
     {
       .text :
       {
         CREATE_OBJECT_SYMBOLS
         *(.text)
          etext  =  .;
          __CTOR_LIST__ = .;
          LONG((__CTOR_END__ - __CTOR_LIST__) / 4 - 2)
         *(.ctors)
          LONG(0)
          __CTOR_END__ = .;
          __DTOR_LIST__ = .;
          LONG((__DTOR_END__ - __DTOR_LIST__) / 4 - 2)
         *(.dtors)
          LONG(0)
          __DTOR_END__ = .;
         *(.lit)
         *(.shdata)
       }  > ram
       .shbss SIZEOF(.text) + ADDR(.text) :	{
         *(.shbss)
       }

   Set up the '.text' section.  In a 'COFF' file, .text is where all the
actual instructions are.  This also sets up the _CONTRUCTOR_ and the
_DESTRUCTOR_ tables for 'G++'.  Notice that the section description
redirects itself to the _ram_ variable setup earlier.

       .talias :	 { }  > ram
       .data  : {
         *(.data)
         CONSTRUCTORS
         _edata  =  .;
       } > ram

   Setup the '.data' section.  In a 'coff' file, this is where all he
initialized data goes.  'CONSTRUCTORS' is a special command used by
'ld'.

       .bss SIZEOF(.data) + ADDR(.data) :
       {
        __bss_start = ALIGN(0x8);
        *(.bss)
        *(COMMON)
           end = ALIGN(0x8);
           _end = ALIGN(0x8);
           __end = ALIGN(0x8);
       }
       .mstack  : { }  > ram
       .rstack  : { }  > ram
       .stab  . (NOLOAD) :
       {
         [ .stab ]
       }
       .stabstr  . (NOLOAD) :
       {
         [ .stabstr ]
       }
     }

   Setup the '.bss' section.  In a 'COFF' file, this is where
unitialized data goes.  The symbols '_bss_start' and '_end' are setup
here for use by the 'crt0.o' when it zero's the '.bss' section.


File: porting.info,  Node: What to do now,  Next: Libc,  Prev: Linker Scripts,  Up: Libraries

3.3 What to do when you have a binary image
===========================================

A few ROM monitors load binary images, typically 'a.out', but most all
will load an 'srecord'.  An srecord is an ASCII representation of a
binary image.  At its simplest, an srecord is an address, followed by a
byte count, followed by the bytes, and a 2's compliment checksum.  A
whole srecord file has an optional _start_ record, and a required _end_
record.  To make an srecord from a binary image, the GNU 'objcopy'
program is used.  This will read the image and make an srecord from it.
To do this, invoke objcopy like this: 'objcopy -O srec infile outfile'.
Most PROM burners also read srecords or a similar format.  Use 'objdump
-i' to get a list of support object files types for your architecture.


File: porting.info,  Node: Libc,  Prev: What to do now,  Up: Libraries

3.4 Libraries
=============

This describes 'newlib', a freely available libc replacement.  Most
applications use calls in the standard C library.  When initially
linking in libc.a, several I/O functions are undefined.  If you don't
plan on doing any I/O, then you're OK, otherwise they need to be
created.  These routines are read, write, open, close.  sbrk, and kill.
Open & close don't need to be fully supported unless you have a
filesystems, so typically they are stubbed out.  Kill is also a stub,
since you can't do process control on an embedded system.

   Sbrk() is only needed by applications that do dynamic memory
allocation.  It uses the symbol '_end' that is setup in the linker
script.  It also requires a compile time option to set the upper size
limit on the heap space.  This leaves us with read and write, which are
required for serial I/O. Usually these two routines are written in C,
and call a lower level function for the actual I/O operation.  These two
lowest level I/O primitives are inbyte() and outbyte(), and are also
used by GDB back ends if you've written an exception handler.  Some
systems also implement a havebyte() for input as well.

   Other commonly included functions are routines for manipulating LED's
on the target (if they exist) or low level debug help.  Typically a
putnum() for printing words and bytes as a hex number is helpful, as
well as a low-level print() to output simple strings.

   As libg++ uses the I/O routines in libc.a, if read and write work,
then libg++ will also work with no additional changes.

* Menu:

* I/O Support::         Functions that make serial I/O work.
* Memory Support::      Memory support.
* Misc Support::        Other needed functions.
* Debugging::            Useful Debugging Functions


File: porting.info,  Node: I/O Support,  Next: Memory Support,  Up: Libc

3.4.1 Making I/O work
---------------------


File: porting.info,  Node: Memory Support,  Next: Misc Support,  Prev: I/O Support,  Up: Libc

3.4.2 Routines for dynamic memory allocation
--------------------------------------------

To support using any of the memory functions, you need to implement
sbrk().  'malloc()', 'calloc()', and 'realloc()' all call 'sbrk()' at
there lowest level.  'caddr_t' is defined elsewhere as 'char *'.
'RAMSIZE' is presently a compile time option.  All this does is move a
pointer to heap memory and check for the upper limit.  *note Example
libc support code: glue.c.  'sbrk()' returns a pointer to the previous
value before more memory was allocated.

     /* _end is set in the linker command file *
     extern caddr_t _end;/

     /* just in case, most boards have at least some memory */
     #ifndef RAMSIZE
     #  define RAMSIZE             (caddr_t)0x100000
     #endif

     /*
      * sbrk -- changes heap size size. Get nbytes more
      *         RAM. We just increment a pointer in what's
      *         left of memory on the board.
      */
     caddr_t
     sbrk(nbytes)
          int nbytes;
     {
       static caddr_t heap_ptr = NULL;
       caddr_t        base;

       if (heap_ptr == NULL) {
         heap_ptr = (caddr_t)&_end;
       }

       if ((RAMSIZE - heap_ptr) >= 0) {
         base = heap_ptr;
         heap_ptr += nbytes;
         return (base);
       } else {
         errno = ENOMEM;
         return ((caddr_t)-1);
       }
     }


File: porting.info,  Node: Misc Support,  Next: Debugging,  Prev: Memory Support,  Up: Libc

3.4.3 Misc support routines
---------------------------

These are called by 'newlib' but don't apply to the embedded
environment.  'isatty()' is self explanatory.  'kill()' doesn't apply
either in an environment withno process control, so it justs exits,
which is a similar enough behavior.  'getpid()' can safely return any
value greater than 1.  The value doesn't effect anything in 'newlib'
because once again there is no process control.

     /*
      * isatty -- returns 1 if connected to a terminal device,
      *           returns 0 if not. Since we're hooked up to a
      *           serial port, we'll say yes and return a 1.
      */
     int
     isatty(fd)
          int fd;
     {
       return (1);
     }

     /*
      * getpid -- only one process, so just return 1.
      */
     #define __MYPID 1
     int
     getpid()
     {
       return __MYPID;
     }

     /*
      * kill -- go out via exit...
      */
     int
     kill(pid, sig)
          int pid;
          int sig;
     {
       if(pid == __MYPID)
         _exit(sig);
       return 0;
     }


File: porting.info,  Node: Debugging,  Prev: Misc Support,  Up: Libc

3.4.4 Useful debugging functions
--------------------------------

There are always a few useful functions for debugging your project in
progress.  I typically implement a simple 'print()' routine that runs
standalone in liblgoss, with no 'newlib' support.  The I/O function
'outbyte()' can also be used for low level debugging.  Many times print
will work when there are problems that cause 'printf()' to cause an
exception.  'putnum()' is just to print out values in hex so they are
easier to read.

     /*
      * print -- do a raw print of a string
      */
     int
     print(ptr)
     char *ptr;
     {
       while (*ptr) {
         outbyte (*ptr++);
       }
     }

     /*
      * putnum -- print a 32 bit number in hex
      */
     int
     putnum (num)
     unsigned int num;
     {
       char  buffer[9];
       int   count;
       char  *bufptr = buffer;
       int   digit;

       for (count = 7 ; count >= 0 ; count--) {
         digit = (num >> (count * 4)) & 0xf;

         if (digit <= 9)
           *bufptr++ = (char) ('0' + digit);
         else
           *bufptr++ = (char) ('a' - 10 + digit);
       }

       *bufptr = (char) 0;
       print (buffer);
       return;
     }

   If there are LEDs on the board, they can also be put to use for
debugging when the serial I/O code is being written.  I usually
implement a 'zylons()' function, which strobes the LEDS (if there is
more than one) in sequence, creating a rotating effect.  This is
convenient between I/O to see if the target is still alive.  Another
useful LED function is 'led_putnum()', which takes a digit and displays
it as a bit pattern or number.  These usually have to be written in
assembler for each target board.  Here are a number of C based routines
that may be useful.

   'led_putnum()' puts a number on a single digit segmented LED display.
This LED is set by setting a bit mask to an address, where 1 turns the
segment off, and 0 turns it on.  There is also a little decimal point on
the LED display, so it gets the leftmost bit.  The other bits specify
the segment location.  The bits look like:

             [d.p | g | f | e | d | c | b | a ] is the byte.

   The locations are set up as:

                  a
                -----
             f |     | b
               |  g  |
                -----
               |     |
             e |     | c
                -----
                  d

   This takes a number that's already been converted to a string, and
prints it.

     #define LED_ADDR	0xd00003

     void
     led_putnum ( num )
     char num;
     {
         static unsigned char *leds = (unsigned char *)LED_ADDR;
         static unsigned char num_bits [18] = {
           0xff,						/* clear all */
           0xc0, 0xf9, 0xa4, 0xb0, 0x99, 0x92, 0x82, 0xf8, 0x80, 0x98, /* numbers 0-9 */
           0x98, 0x20, 0x3, 0x27, 0x21, 0x4, 0xe 		/* letters a-f */
         };

         if (num >= '0' && num <= '9')
           num = (num - '0') + 1;

         if (num >= 'a' && num <= 'f')
           num = (num - 'a') + 12;

         if (num == ' ')
           num = 0;

         *leds = num_bits[num];
     }

     /*
      * zylons -- draw a rotating pattern. NOTE: this function never returns.
      */
     void
     zylons()
     {
       unsigned char *leds 	= (unsigned char *)LED_ADDR;
       unsigned char curled = 0xfe;

       while (1)
         {
           *leds = curled;
           curled = (curled >> 1) | (curled << 7);
           delay ( 200 );
         }
     }


File: porting.info,  Node: GDB,  Next: Binutils,  Prev: Libraries,  Up: Top

4 Writing a new GDB backend
***************************

Typically, either the low-level I/O routines are used for debugging, or
LEDs, if present.  It is much easier to use GDb for debugging an
application.  There are several different techniques used to have GDB
work remotely.  Commonly more than one kind of GDB interface is used to
cober a wide variety of development needs.

   The most common style of GDB backend is an exception handler for
breakpoints.  This is also called a _gdb stub_, and is requires the two
additional lines of init code in your 'main()' routine.  The GDB stubs
all use the GDB _remote protocol_.  When the application gets a
breakpoint exception, it communicates to GDB on the host.

   Another common style of interfacing GDB to a target is by using an
existing ROM monitor.  These break down into two main kinds, a similar
protocol to the GDB remote protocol, and an interface that uses the ROM
monitor directly.  This kind has GDB simulating a human operator, and
all GDB does is work as a command formatter and parser.

* Menu:

* GNU remote protocol::         The standard remote protocol.
* Exception handler::           A linked in exception handler.
* ROM monitors::                Using a ROM monitor as a backend.
* Other remote protocols::      Adding support for new protocols.


File: porting.info,  Node: GNU remote protocol,  Next: Exception handler,  Up: GDB

4.1 The standard remote protocol
================================

The standard remote protocol is a simple, packet based scheme.  A debug
packet whose contents are _<data>_ is encapsulated for transmission in
the form:

     	$ <data> # CSUM1 CSUM2

   _<data>_ must be ASCII alphanumeric and cannot include characters '$'
or '#'.  If _<data>_ starts with two characters followed by ':', then
the existing stubs interpret this as a sequence number.  For example,
the command 'g' is used to read the values of the registers.  So, a
packet to do this would look like

             $g#67

   _CSUM1_ and _CSUM2_ are an ascii representation in hex of an 8-bit
checksum of _<data>_, the most significant nibble is sent first.  the
hex digits 0-9,a-f are used.

   A simple protocol is used when communicating with the target.  This
is mainly to give a degree of error handling over the serial cable.  For
each packet transmitted successfully, the target responds with a '+'
('ACK').  If there was a transmission error, then the target responds
with a '-' ('NAK').  An error is determined when the checksum doesn't
match the calculated checksum for that data record.  Upon reciept of the
'ACK', 'GDB' can then transmit the next packet.

   Here is a list of the main functions that need to be supported.  Each
data packet is a command with a set number of bytes in the command
packet.  Most commands either return data, or respond with a 'NAK'.
Commands that don't return data respond with an 'ACK'.  All data values
are ascii hex digits.  Every byte needs two hex digits to represent t.
This means that a byte with the value '7' becomes '07'.  On a 32 bit
machine this works out to 8 characters per word.  All of the bytes in a
word are stored in the target byte order.  When writing the host side of
the GDB protocol, be careful of byte order, and make sure that the code
will run on both big and little endian hosts and produce the same
answers.

   These functions are the minimum required to make a GDB backend work.
All other commands are optional, and not supported by all GDB backends.

'read registers 'g''

     returns 'XXXXXXXX...'

     Registers are in the internal order for GDB, and the bytes in a
     register are in the same order the machine uses.  All values are in
     sequence starting with register 0.  All registers are listed in the
     same packet.  A sample packet would look like '$g#'.

'write registers	'GXXXXXXXX...''
     'XXXXXXXX' is the value to set the register to.  Registers are in
     the internal order for GDB, and the bytes in a register are in the
     same order the machine uses.  All values are in sequence starting
     with register 0.  All registers values are listed in the same
     packet.  A sample packet would look like
     '$G000000001111111122222222...#'

     returns 'ACK' or 'NAK'

'read memory 'mAAAAAAAA,LLLL''
     'AAAAAAAA' is address, 'LLLL' is length.  A sample packet would
     look like '$m00005556,0024#'.  This would request 24 bytes starting
     at address _00005556_

     returns 'XXXXXXXX...' 'XXXXXXXX' is the memory contents.  Fewer
     bytes than requested will be returned if only part of the data can
     be read.  This can be determined by counting the values till the
     end of packet '#' is seen and comparing that with the total count
     of bytes that was requested.

'write memory	'MAAAAAAAA,LLLL:XXXXXXXX''
     'AAAAAAAA' is the starting address, 'LLLL' is the number of bytes
     to be written, and 'XXXXXXXX' is value to be written.  A sample
     packet would look like
     '$M00005556,0024:101010101111111100000000...#'

     returns 'ACK' or 'NAK' for an error.  'NAK' is also returned when
     only part of the data is written.

'continue	'cAAAAAAAAA''
     'AAAAAAAA' is address to resume execution at.  If 'AAAAAAAA' is
     omitted, resume at the curent address of the 'pc' register.

     returns the same replay as 'last signal'.  There is no immediate
     replay to 'cont' until the next breakpoint is reached, and the
     program stops executing.

'step	sAA..AA'
     'AA..AA' is address to resume If 'AA..AA' is omitted, resume at
     same address.

     returns the same replay as 'last signal'.  There is no immediate
     replay to 'step' until the next breakpoint is reached, and the
     program stops executing.

'last signal '?''

     This returns one of the following:

        * 'SAA' Where 'AA' is the number of the last signal.  Exceptions
          on the target are converted to the most similar Unix style
          signal number, like 'SIGSEGV'.  A sample response of this type
          would look like '$S05#'.

        * TAAnn:XXXXXXXX;nn:XXXXXXXX;nn:XXXXXXXX; 'AA' is the signal
          number.  'nn' is the register number.  'XXXXXXXX' is the
          register value.

        * WAA The process exited, and 'AA' is the exit status.  This is
          only applicable for certains sorts of targets.

     These are used in some GDB backends, but not all.

'write reg 'Pnn=XXXXXXXX''
     Write register 'nn' with value 'XXXXXXXX'.

     returns 'ACK' or 'NAK'

'kill request	k'

'toggle debug	d'
     toggle debug flag (see 386 & 68k stubs)

'reset	r'
     reset - see sparc stub.

'reserved	'other''
     On other requests, the stub should ignore the request and send an
     empty response '$#<checksum>'.  This way we can extend the protocol
     and GDB can tell whether the stub it is	talking to uses the old or
     the new.

'search	'tAA:PP,MM''
     Search backwards starting at address 'AA' for a match with pattern
     PP and mask 'MM'.  'PP' and 'MM' are 4 bytes.

'general query	'qXXXX''
     Request info about XXXX.

'general set	'QXXXX=yyyy''
     Set value of 'XXXX' to 'yyyy'.

'query sect offs	'qOffsets''
     Get section offsets.  Reply is 'Text=xxx;Data=yyy;Bss=zzz'

'console output	Otext'
     Send text to stdout.  The text gets display from the target side of
     the serial connection.

   Responses can be run-length encoded to save space.  A '*'means that
the next character is an ASCII encoding giving a repeat count which
stands for that many repetitions of the character preceding the '*'.
The encoding is n+29, yielding a printable character where n >=3 (which
is where run length encoding starts to win).  You can't use a value of
where n >126 because it's only a two byte value.  An example would be a
'0*03' means the same thing as '0000'.


File: porting.info,  Node: Exception handler,  Next: ROM monitors,  Prev: GNU remote protocol,  Up: GDB

4.2 A linked in exception handler
=================================

A _GDB stub_ consists of two parts, support for the exception handler,
and the exception handler itself.  The exception handler needs to
communicate to GDB on the host whenever there is a breakpoint exception.
When GDB starts a program running on the target, it's polling the serial
port during execution looking for any debug packets.  So when a
breakpoint occurs, the exception handler needs to save state, and send a
GDB remote protocol packet to GDB on the host.  GDB takes any output
that isn't a debug command packet and displays it in the command window.

   Support for the exception handler varies between processors, but the
minimum supported functions are those needed by GDB. These are functions
to support the reading and writing of registers, the reading and writing
of memory, start execution at an address, single step, and last signal.
Sometimes other functions for adjusting the baud rate, or resetting the
hardware are implemented.

   Once GDB gets the command packet from the breakpoint, it will read a
few registers and memory locations an then wait for the user.  When the
user types 'run' or 'continue' a 'continue' command is issued to the
backend, and control returns from the breakpoint routine to the
application.


File: porting.info,  Node: ROM monitors,  Next: Other remote protocols,  Prev: Exception handler,  Up: GDB

4.3 Using a ROM monitor as a backend
====================================

GDB also can mimic a human user and use a ROM monitors normal debug
commands as a backend.  This consists mostly of sending and parsing
'ASCII' strings.  All the ROM monitor interfaces share a common set of
routines in 'gdb/monitor.c'.  This supports adding new ROM monitor
interfaces by filling in a structure with the common commands GDB needs.
GDb already supports several command ROM monitors, including Motorola's
'Bug' monitor for their VME boards, and the Rom68k monitor by Integrated
Systems, Inc.  for various m68k based boards.  GDB also supports the
custom ROM monitors on the WinBond and Oki PA based targets.  There is
builtin support for loading files to ROM monitors specifically.  GDB can
convert a binary into an srecord and then load it as an ascii file, or
using 'xmodem'.


File: porting.info,  Node: Other remote protocols,  Prev: ROM monitors,  Up: GDB

4.4 Adding support for new protocols
====================================


File: porting.info,  Node: Binutils,  Next: Code Listings,  Prev: GDB,  Up: Top


File: porting.info,  Node: Code Listings,  Next: idp.ld,  Prev: Binutils,  Up: Top

Appendix A Code Listings
************************

* Menu:

* idp.ld::              A m68k linker script.
* crt0.S::              Crt0.S for an m68k.
* glue.c::              C based support for for Stdio functions.
* mvme.S::              Rom monitor based I/O support in assembler.
* io.c::                C based for memory mapped I/O.
* leds.c::              C based LED routines.


File: porting.info,  Node: idp.ld,  Next: crt0.S,  Prev: Code Listings,  Up: Code Listings

A.1 Linker script for the IDP board
===================================

This is the linker script script that is used on the Motorola IDP board.

     STARTUP(crt0.o)
     OUTPUT_ARCH(m68k)
     INPUT(idp.o)
     SEARCH_DIR(.)
     __DYNAMIC  =  0;
     /*
      * Setup the memory map of the MC68ec0x0 Board (IDP)
      * stack grows up towards high memory. This works for
      * both the rom68k and the mon68k monitors.
      */
     MEMORY
     {
       ram     : ORIGIN = 0x10000, LENGTH = 2M
     }
     /*
      * stick everything in ram (of course)
      */
     SECTIONS
     {
       .text :
       {
         CREATE_OBJECT_SYMBOLS
         *(.text)
          etext  =  .;
          __CTOR_LIST__ = .;
          LONG((__CTOR_END__ - __CTOR_LIST__) / 4 - 2)
         *(.ctors)
          LONG(0)
          __CTOR_END__ = .;
          __DTOR_LIST__ = .;
          LONG((__DTOR_END__ - __DTOR_LIST__) / 4 - 2)
         *(.dtors)
          LONG(0)
          __DTOR_END__ = .;
         *(.lit)
         *(.shdata)
       }  > ram
       .shbss SIZEOF(.text) + ADDR(.text) :	{
         *(.shbss)
       }
       .talias :	 { }  > ram
       .data  : {
         *(.data)
         CONSTRUCTORS
         _edata  =  .;
       } > ram

       .bss SIZEOF(.data) + ADDR(.data) :
       {
        __bss_start = ALIGN(0x8);
        *(.bss)
        *(COMMON)
           end = ALIGN(0x8);
           _end = ALIGN(0x8);
           __end = ALIGN(0x8);
       }
       .mstack  : { }  > ram
       .rstack  : { }  > ram
       .stab  . (NOLOAD) :
       {
         [ .stab ]
       }
       .stabstr  . (NOLOAD) :
       {
         [ .stabstr ]
       }
     }


File: porting.info,  Node: crt0.S,  Next: glue.c,  Prev: idp.ld,  Up: Code Listings

A.2 crt0.S - The startup file
=============================

     /*
      * crt0.S -- startup file for m68k-coff
      *
      */

     	.title "crt0.S for m68k-coff"

     /* These are predefined by new versions of GNU cpp.  */

     #ifndef __USER_LABEL_PREFIX__
     #define __USER_LABEL_PREFIX__ _
     #endif

     #ifndef __REGISTER_PREFIX__
     #define __REGISTER_PREFIX__
     #endif

     /* ANSI concatenation macros.  */

     #define CONCAT1(a, b) CONCAT2(a, b)
     #define CONCAT2(a, b) a ## b

     /* Use the right prefix for global labels.  */

     #define SYM(x) CONCAT1 (__USER_LABEL_PREFIX__, x)

     /* Use the right prefix for registers.  */

     #define REG(x) CONCAT1 (__REGISTER_PREFIX__, x)

     #define d0 REG (d0)
     #define d1 REG (d1)
     #define d2 REG (d2)
     #define d3 REG (d3)
     #define d4 REG (d4)
     #define d5 REG (d5)
     #define d6 REG (d6)
     #define d7 REG (d7)
     #define a0 REG (a0)
     #define a1 REG (a1)
     #define a2 REG (a2)
     #define a3 REG (a3)
     #define a4 REG (a4)
     #define a5 REG (a5)
     #define a6 REG (a6)
     #define fp REG (fp)
     #define sp REG (sp)

     /*
      * Set up some room for a stack. We just grab a chunk of memory.
      */
     	.set	stack_size, 0x2000
     	.comm	SYM (stack), stack_size

     /*
      * Define an empty environment.
      */
             .data
             .align 2
     SYM (environ):
             .long 0

      	.align	2
     	.text
     	.global SYM (stack)

     	.global SYM (main)
     	.global SYM (exit)
     /*
      * This really should be __bss_start, not SYM (__bss_start).
      */
     	.global __bss_start

     /*
      * start -- set things up so the application will run.
      */
     SYM (start):
     	link	a6, #-8
     	moveal	#SYM (stack) + stack_size, sp

     /*
      * zerobss -- zero out the bss section
      */
     	moveal	#__bss_start, a0
     	moveal	#SYM (end), a1
     1:
     	movel	#0, (a0)
     	leal	4(a0), a0
     	cmpal	a0, a1
     	bne	1b

     /*
      * Call the main routine from the application to get it going.
      * main (argc, argv, environ)
      * We pass argv as a pointer to NULL.
      */
             pea     0
             pea     SYM (environ)
             pea     sp@(4)
             pea     0
     	jsr	SYM (main)
     	movel	d0, sp@-

     /*
      * _exit -- Exit from the application. Normally we cause a user trap
      *          to return to the ROM monitor for another run.
      */
     SYM (exit):
     	trap	#0


File: porting.info,  Node: glue.c,  Next: mvme.S,  Prev: crt0.S,  Up: Code Listings

A.3 C based "glue" code.
========================


     /*
      * glue.c -- all the code to make GCC and the libraries run on
      *           a bare target board. These should work with any
      *           target if inbyte() and outbyte() exist.
      */

     #include <sys/types.h>
     #include <sys/stat.h>
     #include <errno.h>
     #ifndef NULL
     #define NULL 0
     #endif

     /* FIXME: this is a hack till libc builds */
     __main()
     {
       return;
     }

     #undef errno
     int errno;

     extern caddr_t _end;                /* _end is set in the linker command file */
     extern int outbyte();
     extern unsigned char inbyte();
     extern int havebyte();

     /* just in case, most boards have at least some memory */
     #ifndef RAMSIZE
     #  define RAMSIZE             (caddr_t)0x100000
     #endif

     /*
      * read  -- read bytes from the serial port. Ignore fd, since
      *          we only have stdin.
      */
     int
     read(fd, buf, nbytes)
          int fd;
          char *buf;
          int nbytes;
     {
       int i = 0;

       for (i = 0; i < nbytes; i++) {
         *(buf + i) = inbyte();
         if ((*(buf + i) == '\n') || (*(buf + i) == '\r')) {
           (*(buf + i)) = 0;
           break;
         }
       }
       return (i);
     }

     /*
      * write -- write bytes to the serial port. Ignore fd, since
      *          stdout and stderr are the same. Since we have no filesystem,
      *          open will only return an error.
      */
     int
     write(fd, buf, nbytes)
          int fd;
          char *buf;
          int nbytes;
     {
       int i;

       for (i = 0; i < nbytes; i++) {
         if (*(buf + i) == '\n') {
           outbyte ('\r');
         }
         outbyte (*(buf + i));
       }
       return (nbytes);
     }

     /*
      * open -- open a file descriptor. We don't have a filesystem, so
      *         we return an error.
      */
     int
     open(buf, flags, mode)
          char *buf;
          int flags;
          int mode;
     {
       errno = EIO;
       return (-1);
     }

     /*
      * close -- close a file descriptor. We don't need
      *          to do anything, but pretend we did.
      */
     int
     close(fd)
          int fd;
     {
       return (0);
     }

     /*
      * sbrk -- changes heap size size. Get nbytes more
      *         RAM. We just increment a pointer in what's
      *         left of memory on the board.
      */
     caddr_t
     sbrk(nbytes)
          int nbytes;
     {
       static caddr_t heap_ptr = NULL;
       caddr_t        base;

       if (heap_ptr == NULL) {
         heap_ptr = (caddr_t)&_end;
       }

       if ((RAMSIZE - heap_ptr) >= 0) {
         base = heap_ptr;
         heap_ptr += nbytes;
         return (base);
       } else {
         errno = ENOMEM;
         return ((caddr_t)-1);
       }
     }

     /*
      * isatty -- returns 1 if connected to a terminal device,
      *           returns 0 if not. Since we're hooked up to a
      *           serial port, we'll say yes and return a 1.
      */
     int
     isatty(fd)
          int fd;
     {
       return (1);
     }

     /*
      * lseek -- move read/write pointer. Since a serial port
      *          is non-seekable, we return an error.
      */
     off_t
     lseek(fd,  offset, whence)
          int fd;
          off_t offset;
          int whence;
     {
       errno = ESPIPE;
       return ((off_t)-1);
     }

     /*
      * fstat -- get status of a file. Since we have no file
      *          system, we just return an error.
      */
     int
     fstat(fd, buf)
          int fd;
          struct stat *buf;
     {
       errno = EIO;
       return (-1);
     }

     /*
      * getpid -- only one process, so just return 1.
      */
     #define __MYPID 1
     int
     getpid()
     {
       return __MYPID;
     }

     /*
      * kill -- go out via exit...
      */
     int
     kill(pid, sig)
          int pid;
          int sig;
     {
       if(pid == __MYPID)
         _exit(sig);
       return 0;
     }

     /*
      * print -- do a raw print of a string
      */
     int
     print(ptr)
     char *ptr;
     {
       while (*ptr) {
         outbyte (*ptr++);
       }
     }

     /*
      * putnum -- print a 32 bit number in hex
      */
     int
     putnum (num)
     unsigned int num;
     {
       char  buffer[9];
       int   count;
       char  *bufptr = buffer;
       int   digit;

       for (count = 7 ; count >= 0 ; count--) {
         digit = (num >> (count * 4)) & 0xf;

         if (digit <= 9)
           *bufptr++ = (char) ('0' + digit);
         else
           *bufptr++ = (char) ('a' - 10 + digit);
       }

       *bufptr = (char) 0;
       print (buffer);
       return;
     }


File: porting.info,  Node: mvme.S,  Next: io.c,  Prev: glue.c,  Up: Code Listings

A.4 I/O assembler code sample
=============================

     /*
      * mvme.S -- board support for m68k
      */

     	.title "mvme.S for m68k-coff"

     /* These are predefined by new versions of GNU cpp.  */

     #ifndef __USER_LABEL_PREFIX__
     #define __USER_LABEL_PREFIX__ _
     #endif

     #ifndef __REGISTER_PREFIX__
     #define __REGISTER_PREFIX__
     #endif

     /* ANSI concatenation macros.  */

     #define CONCAT1(a, b) CONCAT2(a, b)
     #define CONCAT2(a, b) a ## b

     /* Use the right prefix for global labels.  */

     #define SYM(x) CONCAT1 (__USER_LABEL_PREFIX__, x)

     /* Use the right prefix for registers.  */

     #define REG(x) CONCAT1 (__REGISTER_PREFIX__, x)

     #define d0 REG (d0)
     #define d1 REG (d1)
     #define d2 REG (d2)
     #define d3 REG (d3)
     #define d4 REG (d4)
     #define d5 REG (d5)
     #define d6 REG (d6)
     #define d7 REG (d7)
     #define a0 REG (a0)
     #define a1 REG (a1)
     #define a2 REG (a2)
     #define a3 REG (a3)
     #define a4 REG (a4)
     #define a5 REG (a5)
     #define a6 REG (a6)
     #define fp REG (fp)
     #define sp REG (sp)
     #define vbr REG (vbr)

     	.align	2
     	.text
     	.global SYM (_exit)
     	.global SYM (outln)
     	.global SYM (outbyte)
     	.global SYM (putDebugChar)
     	.global SYM (inbyte)
     	.global SYM (getDebugChar)
     	.global SYM (havebyte)
     	.global SYM (exceptionHandler)

     	.set	vbr_size, 0x400
     	.comm	SYM (vbr_table), vbr_size

     /*
      * inbyte -- get a byte from the serial port
      *	d0 - contains the byte read in
      */
     	.align	2
     SYM (getDebugChar):		/* symbol name used by m68k-stub */
     SYM (inbyte):
     	link	a6, #-8
     	trap 	#15
     	.word	inchr
     	moveb 	sp@, d0
     	extbl	d0
     	unlk	a6
     	rts

     /*
      * outbyte -- sends a byte out the serial port
      *	d0 - contains the byte to be sent
      */
     	.align	2
     SYM (putDebugChar):		/* symbol name used by m68k-stub */
     SYM (outbyte):
     	link	fp, #-4
      	moveb	fp@(11), sp@
     	trap 	#15
     	.word	outchr
     	unlk	fp
     	rts

     /*
      * outln -- sends a string of bytes out the serial port with a CR/LF
      *	a0 - contains the address of the string's first byte
      *	a1 - contains the address of the string's last byte
      */
     	.align	2
     SYM (outln):
     	link	a6, #-8
     	moveml	a0/a1, sp@
     	trap 	#15
     	.word 	outln
     	unlk	a6
     	rts

     /*
      * outstr -- sends a string of bytes out the serial port without a CR/LF
      *	a0 - contains the address of the string's first byte
      *	a1 - contains the address of the string's last byte
      */
     	.align	2
     SYM (outstr):
     	link	a6, #-8
     	moveml	a0/a1, sp@
     	trap 	#15
     	.word 	outstr
     	unlk	a6
     	rts

     /*
      * havebyte -- checks to see if there is a byte in the serial port,
      *	     returns 1 if there is a byte, 0 otherwise.
      */
     SYM (havebyte):
     	trap 	#15
     	.word	instat
     	beqs	empty
     	movel 	#1, d0
     	rts
     empty:
     	movel	#0, d0
     	rts

     /*
      * These constants are for the MVME-135 board's boot monitor. They
      * are used with a TRAP #15 call to access the monitor's I/O routines.
      * they must be in the word following the trap call.
      */
     	.set inchr, 0x0
     	.set instat, 0x1
     	.set inln, 0x2
     	.set readstr, 0x3
     	.set readln, 0x4
     	.set chkbrk, 0x5

     	.set outchr, 0x20
     	.set outstr, 0x21
     	.set outln, 0x22
     	.set write, 0x23
     	.set writeln, 0x24
     	.set writdln, 0x25
     	.set pcrlf, 0x26
     	.set eraseln, 0x27
     	.set writd, 0x28
     	.set sndbrk, 0x29

     	.set tm_ini, 0x40
     	.set dt_ini, 0x42
     	.set tm_disp, 0x43
     	.set tm_rd, 0x44

     	.set redir, 0x60
     	.set redir_i, 0x61
     	.set redir_o, 0x62
     	.set return, 0x63
     	.set bindec, 0x64

     	.set changev, 0x67
     	.set strcmp, 0x68
     	.set mulu32, 0x69
     	.set divu32, 0x6A
     	.set chk_sum, 0x6B



File: porting.info,  Node: io.c,  Next: leds.c,  Prev: mvme.S,  Up: Code Listings

A.5 I/O code sample
===================

     #include "w89k.h"

     /*
      * outbyte -- shove a byte out the serial port. We wait till the byte
      */
     int
     outbyte(byte)
          unsigned char byte;
     {
       while ((inp(RS232REG) & TRANSMIT) == 0x0) {  } ;
       return (outp(RS232PORT, byte));
     }

     /*
      * inbyte -- get a byte from the serial port
      */
     unsigned char
     inbyte()
     {
       while ((inp(RS232REG) & RECEIVE) == 0x0) { };
       return (inp(RS232PORT));
     }


File: porting.info,  Node: leds.c,  Prev: io.c,  Up: Code Listings

A.6 Led control sample
======================

     /*
      * leds.h -- control the led's on a Motorola mc68ec0x0 board.
      */

     #ifndef __LEDS_H__
     #define __LEDS_H__

     #define LED_ADDR	0xd00003
     #define LED_0           ~0x1
     #define LED_1           ~0x2
     #define LED_2           ~0x4
     #define LED_3           ~0x8
     #define LED_4           ~0x10
     #define LED_5           ~0x20
     #define LED_6           ~0x40
     #define LED_7           ~0x80
     #define LEDS_OFF	0xff
     #define LEDS_ON		0x0

     #define FUDGE(x) ((x >= 0xa && x <= 0xf) ? (x + 'a') & 0x7f : (x + '0') & 0x7f)

     extern void led_putnum( char );

     #endif		/* __LEDS_H__ */

     /*
      * leds.c -- control the led's on a Motorola mc68ec0x0 (IDP)board.
      */
     #include "leds.h"

     void zylons();
     void led_putnum();

     /*
      * led_putnum -- print a hex number on the LED. the value of num must be a char with
      *              the ascii value. ie... number 0 is '0', a is 'a', ' ' (null) clears
      *		the led display.
      *		Setting the bit to 0 turns it on, 1 turns it off.
      * 		the LED's are controlled by setting the right bit mask in the base
      * 		address.
      *		The bits are:
      *			[d.p | g | f | e | d | c | b | a ] is the byte.
      *
      *		The locations are:
      *
      *			 a
      *		       -----
      *		    f |     | b
      *		      |  g  |
      *		       -----
      *                    |     |
      *                  e |     | c
      *                     -----
      *                       d                . d.p (decimal point)
      */
     void
     led_putnum ( num )
     char num;
     {
         static unsigned char *leds = (unsigned char *)LED_ADDR;
         static unsigned char num_bits [18] = {
           0xff,						/* clear all */
           0xc0, 0xf9, 0xa4, 0xb0, 0x99, 0x92, 0x82, 0xf8, 0x80, 0x98, /* numbers 0-9 */
           0x98, 0x20, 0x3, 0x27, 0x21, 0x4, 0xe 		/* letters a-f */
         };

         if (num >= '0' && num <= '9')
           num = (num - '0') + 1;

         if (num >= 'a' && num <= 'f')
           num = (num - 'a') + 12;

         if (num == ' ')
           num = 0;

         *leds = num_bits[num];
     }

     /*
      * zylons -- draw a rotating pattern. NOTE: this function never returns.
      */
     void
     zylons()
     {
       unsigned char *leds 	= (unsigned char *)LED_ADDR;
       unsigned char curled = 0xfe;

       while (1)
         {
           *leds = curled;
           curled = (curled >> 1) | (curled << 7);
           delay ( 200 );
         }
     }



Tag Table:
Node: Top1447
Node: Libgloss2234
Node: Supported targets5410
Node: Blackfin5946
Node: Sparclite6221
Node: CPU327143
Node: Mips8443
Node: PA-RISC9761
Node: Building libgloss11290
Node: Board support14899
Node: Build System Internals17039
Node: GCC19342
Node: Overview20633
Node: Options22861
Node: GCC Options23537
Node: GAS Options23832
Node: LD Options23927
Node: Libraries24002
Node: Crt024314
Node: Linker Scripts30577
Node: What to do now35436
Node: Libc36329
Node: I/O Support38177
Node: Memory Support38298
Node: Misc Support39758
Node: Debugging40931
Node: GDB44502
Node: GNU remote protocol45902
Node: Exception handler52404
Node: ROM monitors53823
Node: Other remote protocols54801
Node: Binutils54960
Node: Code Listings55043
Node: idp.ld55514
Node: crt0.S57261
Node: glue.c59864
Node: mvme.S64752
Node: io.c68899
Node: leds.c69509

End Tag Table


Local Variables:
coding: utf-8
End:
