Next: MicroBlaze Options, Previous: M680x0 Options, Up: Submodel Options [Contents][Index]

#### 3.19.26 MCore Options

These are the ‘`-m`’ options defined for the Motorola M*Core processors.

`-mhardlit`
`-mno-hardlit`

  Inline constants into the code stream if it can be done in two instructions or less.

`-mdiv`
`-mno-div`

  Use the divide instruction. (Enabled by default).

`-mrelax-immediate`
`-mno-relax-immediate`

  Allow arbitrary-sized immediates in bit operations.

`-mwide-bitfields`
`-mno-wide-bitfields`

  Always treat bit-fields as `int`-sized.

`-m4byte-functions`
`-mno-4byte-functions`

  Force all functions to be aligned to a 4-byte boundary.

`-mcallgraph-data`
`-mno-callgraph-data`

  Emit callgraph information.

`-mslow-bytes`
`-mno-slow-bytes`

  Prefer word access when reading byte quantities.

`-mlittle-endian`
`-mbig-endian`

  Generate code for a little-endian target.

`-m210`
`-m340`

  Generate code for the 210 processor.

`-mno-lsim`

  Assume that runtime support has been provided and so omit the simulator library (`libsim.a)` from the linker command line.

`-mstack-increment=size`

  Set the maximum amount for a single stack increment operation. Large values can increase the speed of programs that contain functions that need a large amount of stack space, but they can also trigger a segmentation fault if the stack is extended too much. The default value is 0x1000.