CMSIS-DAP V2 USB WinUSB Firmware for NXP LPC-Link-II board.

CMSIS-DAP with default V2 configuration uses WinUSB interface to host PC and is therefore faster. 
Optionally support for streaming SWO trace is provided via an additional USB endpoint.