Next: ARC Function Attributes, Previous: AArch64 Function Attributes, Up: Function Attributes [Contents][Index]

#### 6.33.3 AMD GCN Function Attributes

These function attributes are supported by the AMD GCN back end:

`amdgpu_hsa_kernel`

  This attribute indicates that the corresponding function should be compiled as a kernel function, that is an entry point that can be invoked from the host via the HSA runtime library. By default functions are only callable only from other GCN functions.

  This attribute is implicitly applied to any function named `main`, using default parameters.

  Kernel functions may return an integer value, which will be written to a conventional place within the HSA "kernargs" region.

  The attribute parameters configure what values are passed into the kernel function by the GPU drivers, via the initial register state. Some values are used by the compiler, and therefore forced on. Enabling other options may break assumptions in the compiler and/or run-time libraries.

  `private_segment_buffer`

    Set `enable_sgpr_private_segment_buffer` flag. Always on (required to locate the stack).

  `dispatch_ptr`

    Set `enable_sgpr_dispatch_ptr` flag. Always on (required to locate the launch dimensions).

  `queue_ptr`

    Set `enable_sgpr_queue_ptr` flag. Always on (required to convert address spaces).

  `kernarg_segment_ptr`

    Set `enable_sgpr_kernarg_segment_ptr` flag. Always on (required to locate the kernel arguments, "kernargs").

  `dispatch_id`

    Set `enable_sgpr_dispatch_id` flag.

  `flat_scratch_init`

    Set `enable_sgpr_flat_scratch_init` flag.

  `private_segment_size`

    Set `enable_sgpr_private_segment_size` flag.

  `grid_workgroup_count_X`

    Set `enable_sgpr_grid_workgroup_count_x` flag. Always on (required to use OpenACC/OpenMP).

  `grid_workgroup_count_Y`

    Set `enable_sgpr_grid_workgroup_count_y` flag.

  `grid_workgroup_count_Z`

    Set `enable_sgpr_grid_workgroup_count_z` flag.

  `workgroup_id_X`

    Set `enable_sgpr_workgroup_id_x` flag.

  `workgroup_id_Y`

    Set `enable_sgpr_workgroup_id_y` flag.

  `workgroup_id_Z`

    Set `enable_sgpr_workgroup_id_z` flag.

  `workgroup_info`

    Set `enable_sgpr_workgroup_info` flag.

  `private_segment_wave_offset`

    Set `enable_sgpr_private_segment_wave_byte_offset` flag. Always on (required to locate the stack).

  `work_item_id_X`

    Set `enable_vgpr_workitem_id` parameter. Always on (can’t be disabled).

  `work_item_id_Y`

    Set `enable_vgpr_workitem_id` parameter. Always on (required to enable vectorization.)

  `work_item_id_Z`

    Set `enable_vgpr_workitem_id` parameter. Always on (required to use OpenACC/OpenMP).

Next: ARC Function Attributes, Previous: AArch64 Function Attributes, Up: Function Attributes [Contents][Index]